--- a/drivers/leds/trigger/Kconfig
+++ b/drivers/leds/trigger/Kconfig
@@ -108,4 +108,11 @@ config LEDS_TRIGGER_CAMERA
 	  This enables direct flash/torch on/off by the driver, kernel space.
 	  If unsure, say Y.
 
+config LEDS_TRIGGER_NETDEV
+	tristate "LED Netdev Trigger"
+	depends on NET && LEDS_TRIGGERS
+	help
+	  This allows LEDs to be controlled by network device activity.
+	  If unsure, say Y.
+
 endif # LEDS_TRIGGERS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -62,3 +62,4 @@ obj-$(CONFIG_LEDS_DAC124S085)		+= leds-d
 
 # LED Triggers
 obj-$(CONFIG_LEDS_TRIGGERS)		+= trigger/
+obj-$(CONFIG_LEDS_TRIGGER_NETDEV)	+= ledtrig-netdev.o
