/dts-v1/;

#include "mt7620a.dtsi"
#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "ralink,mt7620a-soc";
	model = "TP-Link Archer MR200";

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	gpio-leds {
		compatible = "gpio-leds";

		lan {
			label = "mr200:white:lan";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
		};

		wan {
			label = "mr200:white:wan";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		power {
			label = "mr200:white:power";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		4g {
			label = "mr200:white:4g";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "mr200:white:wps";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};

		signal1 {
			label = "mr200:white:signal1";
			gpios = <&gpio2 1 GPIO_ACTIVE_LOW>;
		};

		signal2 {
			label = "mr200:white:signal2";
			gpios = <&gpio2 2 GPIO_ACTIVE_LOW>;
		};

		signal3 {
			label = "mr200:white:signal3";
			gpios = <&gpio2 3 GPIO_ACTIVE_LOW>;
		};

		signal4 {
			label = "mr200:white:signal4";
			gpios = <&gpio2 4 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "mr200:white:wlan";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";
		#address-cells = <1>;
		#size-cells = <0>;

		reset {
			label = "reset";
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};

		rfkill {
			label = "rfkill";
			gpios = <&gpio0 9 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RFKILL>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		power_usb {
			gpio-export,name = "power_usb1";
			gpio-export,output = <1>;
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};
	};

};

&gpio1 {
	status = "okay";
};

&gpio2 {
	status = "okay";
};

&gpio3 {
	status = "okay";
};

&spi0 {
	status = "okay";

	m25p80@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		linux,modalias = "m25p80", "mx25l6405d";
		spi-max-frequency = <10000000>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x20000>;
			read-only;
		};

		partition@20000 {
			label = "firmware";
			reg = <0x20000 0x7b0000>;
		};

		rom: partition@7d0000 {
			label = "rom";
			reg = <0x7d0000 0x10000>;
			read-only;
		};

		partition@7e0000 {
			label = "romfile";
			reg = <0x7e0000 0x10000>;
			read-only;
		};

		radio: partition@7f0000 {
			label = "radio";
			reg = <0x7f0000 0x10000>;
			read-only;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "uartf", "rgmii1", "rgmii2", "wled", "nd_sd", "ephy", "spi refclk";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
		mtd-mac-address = <&rom 0xf100>;
		mediatek,portmap = "llll";
	};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&gsw {
	mediatek,port4 = "ephy";
};

&wmac {
	ralink,mtd-eeprom = <&radio 0>;
};

&pcie {
	status = "okay";

	pcie-bridge {
		mt76@0,0 {
			reg = <0x0000 0 0 0 0>;
			device_type = "pci";
			mediatek,mtd-eeprom = <&radio 32768>;
			mediatek,2ghz = <0>;
		};
	};
};
