From d7146829c9da24e285cb1b1f2156b5b3e2d40c07 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Thu, 19 May 2016 22:07:34 +0200
Subject: [PATCH] MIPS: ralink: fix MT7628 pinmux typos
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Cc: john@phrozen.org
Cc: linux-mips@linux-mips.org
Cc: linux-kernel@vger.kernel.org
Patchwork: https://patchwork.linux-mips.org/patch/13306/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ralink/mt7620.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/mips/ralink/mt7620.c
+++ b/arch/mips/ralink/mt7620.c
@@ -223,9 +223,9 @@ static struct rt2880_pmx_func wled_an_gr
 #define MT7628_GPIO_MODE_GPIO		0
 
 static struct rt2880_pmx_group mt7628an_pinmux_data[] = {
-	GRP_G("pmw1", pwm1_grp_mt7628, MT7628_GPIO_MODE_MASK,
+	GRP_G("pwm1", pwm1_grp_mt7628, MT7628_GPIO_MODE_MASK,
 				1, MT7628_GPIO_MODE_PWM1),
-	GRP_G("pmw0", pwm0_grp_mt7628, MT7628_GPIO_MODE_MASK,
+	GRP_G("pwm0", pwm0_grp_mt7628, MT7628_GPIO_MODE_MASK,
 				1, MT7628_GPIO_MODE_PWM0),
 	GRP_G("uart2", uart2_grp_mt7628, MT7628_GPIO_MODE_MASK,
 				1, MT7628_GPIO_MODE_UART2),
