From 0cc774ef2524ec54e9d2db8771ba3739cb8ebc99 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Mon, 13 Jan 2014 11:08:47 +0100
Subject: [PATCH] ARM: sun5i: a13: Add missing serial aliases

Some UART aliases have been defined, but not all of them. Add the remaining
ones to be consistent and to ease the parsing of the DT by the bootloaders.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun5i-a13.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm/boot/dts/sun5i-a13.dtsi b/arch/arm/boot/dts/sun5i-a13.dtsi
index 320335a..6de40b6 100644
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -16,6 +16,11 @@
 / {
 	interrupt-parent = <&intc>;
 
+	aliases {
+		serial0 = &uart1;
+		serial1 = &uart3;
+	};
+
 	cpus {
 		#address-cells = <1>;
 		#size-cells = <0>;
-- 
1.8.5.5

