From b3cb099f8b0cbe56fcfbb4fb9c7cce48afff41f0 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Emilio=20L=C3=B3pez?= <emilio@elopez.com.ar>
Date: Fri, 20 Sep 2013 22:03:10 -0300
Subject: [PATCH] clk: sunxi: factors: fix off-by-one masks
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The previous code would generate one bit too long masks, and was
needlessly complicated. This patch replaces it by simpler code that can
generate the masks correctly.

Signed-off-by: Emilio López <emilio@elopez.com.ar>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 drivers/clk/sunxi/clk-factors.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/clk/sunxi/clk-factors.c
+++ b/drivers/clk/sunxi/clk-factors.c
@@ -40,7 +40,7 @@ struct clk_factors {
 
 #define to_clk_factors(_hw) container_of(_hw, struct clk_factors, hw)
 
-#define SETMASK(len, pos)		(((-1U) >> (31-len))  << (pos))
+#define SETMASK(len, pos)		(((1U << (len)) - 1) << (pos))
 #define CLRMASK(len, pos)		(~(SETMASK(len, pos)))
 #define FACTOR_GET(bit, len, reg)	(((reg) & SETMASK(len, bit)) >> (bit))
 
