From 64c3866d232e6b29862f4773ea97b16f4dad6950 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Thu, 2 Jan 2014 22:05:04 +0100
Subject: [PATCH] ARM: sun5i: a10s: Add missing serial aliases

Some UART aliases have been defined, but not all of them. Add the remaining
ones to be consistent and to ease the parsing of the DT by the bootloaders.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun5i-a10s.dtsi | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm/boot/dts/sun5i-a10s.dtsi b/arch/arm/boot/dts/sun5i-a10s.dtsi
index 6496159..e00f292 100644
--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -18,6 +18,10 @@
 
 	aliases {
 		ethernet0 = &emac;
+		serial0 = &uart0;
+		serial1 = &uart1;
+		serial2 = &uart2;
+		serial3 = &uart3;
 	};
 
 	cpus {
-- 
1.8.5.5

