From: Felix Fietkau <nbd@openwrt.org>
Date: Sat, 27 Sep 2014 15:58:51 +0200
Subject: [PATCH] ath5k: fix AHB kconfig dependency

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
---

--- a/drivers/net/wireless/ath/ath5k/Kconfig
+++ b/drivers/net/wireless/ath/ath5k/Kconfig
@@ -7,8 +7,8 @@ config ATH5K
 	select BACKPORT_LEDS_CLASS
 	select BACKPORT_NEW_LEDS
 	select BACKPORT_AVERAGE
-	select ATH5K_AHB if (ATHEROS_AR231X && !PCI)
-	select ATH5K_PCI if (!ATHEROS_AR231X && PCI)
+	select ATH5K_AHB if ATHEROS_AR231X
+	select ATH5K_PCI if !ATHEROS_AR231X
 	---help---
 	  This module adds support for wireless adapters based on
 	  Atheros 5xxx chipset.
@@ -55,14 +55,14 @@ config ATH5K_TRACER
 
 config ATH5K_AHB
 	bool "Atheros 5xxx AHB bus support"
-	depends on (ATHEROS_AR231X && !PCI)
+	depends on ATHEROS_AR231X
 	---help---
 	  This adds support for WiSoC type chipsets of the 5xxx Atheros
 	  family.
 
 config ATH5K_PCI
 	bool "Atheros 5xxx PCI bus support"
-	depends on (!ATHEROS_AR231X && PCI)
+	depends on !ATHEROS_AR231X
 	---help---
 	  This adds support for PCI type chipsets of the 5xxx Atheros
 	  family.
