From 172230195068703b78ad5733a09492f5d6814c09 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Tue, 28 Feb 2017 14:15:50 +0100
Subject: [PATCH] ARM: dts: armada: Add default trigger for sata led

In others board we have the sata led set to function
with the sata led trigger by default.
This patch makes the same for these board that have sata
led but get disabled by not associating it to any trigger.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Acked-by: Jason Cooper <jason@lakedaemon.net>
Signed-off-by: Gregory CLEMENT <gregory.clement@free-electrons.com>
---
 arch/arm/boot/dts/armada-385-linksys-caiman.dts | 1 +
 arch/arm/boot/dts/armada-385-linksys-cobra.dts  | 1 +
 arch/arm/boot/dts/armada-xp-linksys-mamba.dts   | 1 +
 3 files changed, 3 insertions(+)

--- a/arch/arm/boot/dts/armada-385-linksys-caiman.dts
+++ b/arch/arm/boot/dts/armada-385-linksys-caiman.dts
@@ -100,6 +100,7 @@
 
 	sata {
 		label = "caiman:white:sata";
+		linux,default-trigger = "disk-activity";
 	};
 };
 
--- a/arch/arm/boot/dts/armada-385-linksys-cobra.dts
+++ b/arch/arm/boot/dts/armada-385-linksys-cobra.dts
@@ -100,6 +100,7 @@
 
 	sata {
 		label = "cobra:white:sata";
+		linux,default-trigger = "disk-activity";
 	};
 };
 
