From cb9bea773c85e372931cd7a177db4165adf29d95 Mon Sep 17 00:00:00 2001
From: Aloka Dixit <quic_alokad@quicinc.com>
Date: Fri, 5 May 2023 16:11:28 +0300
Subject: [PATCH 75/77] wifi: ath11k: refactor vif parameter configurations

Security parameters for each non-transmitting profile can be
different when MBSSID is enabled and this information is included
in the MBSSID element in the Beacon frame. Current implementation
to set rsnie_present and wpaie_present does not parse this element
hence it applies only to the transmitting interface.

Move the code to a separate function to make additions for
non-transmitting interfaces cleaner.

Tested-on: IPQ8074 hw2.0 AHB WLAN.HK.2.7.0.1-01744-QCAHKSWPL_SILICONZ-1

Signed-off-by: Aloka Dixit <quic_alokad@quicinc.com>
Signed-off-by: Kalle Valo <quic_kvalo@quicinc.com>
Link: https://lore.kernel.org/r/20230405221648.17950-6-quic_alokad@quicinc.com
---
 drivers/net/wireless/ath/ath11k/mac.c | 41 ++++++++++++++++-----------
 1 file changed, 24 insertions(+), 17 deletions(-)

--- a/drivers/net/wireless/ath/ath11k/mac.c
+++ b/drivers/net/wireless/ath/ath11k/mac.c
@@ -1351,28 +1351,14 @@ err_mon_del:
 	return ret;
 }
 
-static int ath11k_mac_setup_bcn_tmpl(struct ath11k_vif *arvif)
+static void ath11k_mac_set_vif_params(struct ath11k_vif *arvif,
+				      struct sk_buff *bcn)
 {
-	struct ath11k *ar = arvif->ar;
-	struct ath11k_base *ab = ar->ab;
-	struct ieee80211_hw *hw = ar->hw;
-	struct ieee80211_vif *vif = arvif->vif;
-	struct ieee80211_mutable_offsets offs = {};
-	struct sk_buff *bcn;
 	struct ieee80211_mgmt *mgmt;
 	u8 *ies;
-	int ret;
-
-	if (arvif->vdev_type != WMI_VDEV_TYPE_AP)
-		return 0;
-
-	bcn = ieee80211_beacon_get_template(hw, vif, &offs, 0);
-	if (!bcn) {
-		ath11k_warn(ab, "failed to get beacon template from mac80211\n");
-		return -EPERM;
-	}
 
 	ies = bcn->data + ieee80211_get_hdrlen_from_skb(bcn);
+	mgmt = (struct ieee80211_mgmt *)bcn->data;
 	ies += sizeof(mgmt->u.beacon);
 
 	if (cfg80211_find_ie(WLAN_EID_RSN, ies, (skb_tail_pointer(bcn) - ies)))
@@ -1386,7 +1372,28 @@ static int ath11k_mac_setup_bcn_tmpl(str
 		arvif->wpaie_present = true;
 	else
 		arvif->wpaie_present = false;
+}
+
+static int ath11k_mac_setup_bcn_tmpl(struct ath11k_vif *arvif)
+{
+	struct ath11k *ar = arvif->ar;
+	struct ath11k_base *ab = ar->ab;
+	struct ieee80211_hw *hw = ar->hw;
+	struct ieee80211_vif *vif = arvif->vif;
+	struct ieee80211_mutable_offsets offs = {};
+	struct sk_buff *bcn;
+	int ret;
+
+	if (arvif->vdev_type != WMI_VDEV_TYPE_AP)
+		return 0;
+
+	bcn = ieee80211_beacon_get_template(hw, vif, &offs, 0);
+	if (!bcn) {
+		ath11k_warn(ab, "failed to get beacon template from mac80211\n");
+		return -EPERM;
+	}
 
+	ath11k_mac_set_vif_params(arvif, bcn);
 	ret = ath11k_wmi_bcn_tmpl(ar, arvif->vdev_id, &offs, bcn);
 
 	kfree_skb(bcn);
