From 703d6551f71e7290619d6effe2a25a64e10538b7 Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Thu, 15 Dec 2022 12:20:52 +0100
Subject: [PATCH] ath11k: control thermal support via symbol

Currently, thermal support will get built if CONFIG_THERMAL is reachable,
however this is not suitable for libreCMC as with ALL_KMODS being set to y
ATH11K_THERMAL wont get selected and so hwmon and thermal kmods wont get
pulled in resulting in a build-failure.

So, to avoid that, lets do what is already done for ath10k and add a
config symbol into backports for enabling thermal support.

Signed-off-by: Robert Marko <robimarko@gmail.com>
---
 drivers/net/wireless/ath/ath11k/Kconfig   | 7 +++++++
 drivers/net/wireless/ath/ath11k/Makefile  | 2 +-
 drivers/net/wireless/ath/ath11k/thermal.h | 2 +-
 local-symbols                             | 1 +
 4 files changed, 10 insertions(+), 2 deletions(-)

--- a/drivers/net/wireless/ath/ath11k/Kconfig
+++ b/drivers/net/wireless/ath/ath11k/Kconfig
@@ -61,3 +61,10 @@ config ATH11K_SPECTRAL
 	  Enable ath11k spectral scan support
 
 	  Say Y to enable access to the FFT/spectral data via debugfs.
+
+config ATH11K_THERMAL
+	bool "ath11k thermal sensors and throttling support"
+	depends on ATH11K
+	depends on THERMAL
+	help
+	  Enable ath11k thermal sensors and throttling support.
--- a/drivers/net/wireless/ath/ath11k/Makefile
+++ b/drivers/net/wireless/ath/ath11k/Makefile
@@ -22,7 +22,7 @@ ath11k-y += core.o \
 ath11k-$(CPTCFG_ATH11K_DEBUGFS) += debugfs.o debugfs_htt_stats.o debugfs_sta.o
 ath11k-$(CPTCFG_NL80211_TESTMODE) += testmode.o
 ath11k-$(CPTCFG_ATH11K_TRACING) += trace.o
-ath11k-$(CONFIG_THERMAL) += thermal.o
+ath11k-$(CPTCFG_ATH11K_THERMAL) += thermal.o
 ath11k-$(CPTCFG_ATH11K_SPECTRAL) += spectral.o
 ath11k-$(CONFIG_PM) += wow.o
 
--- a/drivers/net/wireless/ath/ath11k/thermal.h
+++ b/drivers/net/wireless/ath/ath11k/thermal.h
@@ -25,7 +25,7 @@ struct ath11k_thermal {
 	int temperature;
 };
 
-#if IS_REACHABLE(CONFIG_THERMAL)
+#if IS_REACHABLE(CPTCFG_ATH11K_THERMAL)
 int ath11k_thermal_register(struct ath11k_base *sc);
 void ath11k_thermal_unregister(struct ath11k_base *sc);
 int ath11k_thermal_set_throttling(struct ath11k *ar, u32 throttle_state);
--- a/local-symbols
+++ b/local-symbols
@@ -174,6 +174,7 @@ ATH11K_DEBUG=
 ATH11K_DEBUGFS=
 ATH11K_TRACING=
 ATH11K_SPECTRAL=
+ATH11K_THERMAL=
 WLAN_VENDOR_ATMEL=
 ATMEL=
 PCI_ATMEL=
