From d2314a5265eb43e754a26050caa2b31527cc1770 Mon Sep 17 00:00:00 2001
From: Ding Tao <miyatsu@qq.com>
Date: Fri, 26 Oct 2018 11:50:27 +0000
Subject: [PATCH] arm64: dts: marvell: armada37xx: Add emmc/sdio pinctrl
 definition

Add emmc/sdio pinctrl definition for marvell armada37xx SoCs.

Signed-off-by: Ding Tao <miyatsu@qq.com>
Signed-off-by: Gregory CLEMENT <gregory.clement@bootlin.com>
---
 arch/arm64/boot/dts/marvell/armada-37xx.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/arch/arm64/boot/dts/marvell/armada-37xx.dtsi
+++ b/arch/arm64/boot/dts/marvell/armada-37xx.dtsi
@@ -218,6 +218,11 @@
 					groups = "uart2";
 					function = "uart";
 				};
+
+				mmc_pins: mmc-pins {
+					groups = "emmc_nb";
+					function = "emmc";
+				};
 			};
 
 			nb_pm: syscon@14000 {
@@ -247,6 +252,11 @@
 					function = "mii";
 				};
 
+				sdio_pins: sdio-pins {
+					groups = "sdio_sb";
+					function = "sdio";
+				};
+
 				pcie_reset_pins: pcie-reset-pins {
 					groups = "pcie1";
 					function = "gpio";
