From e1dbe9ecf621b6f71f3d2df3e50731d583f3d27f Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Fri, 27 Aug 2021 11:27:53 +0200
Subject: [PATCH] phy: marvell: phy-mvebu-a3700-comphy: Remove unsupported
 modes
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Armada 3700 does not support RXAUI, XFI and neither SFI. Remove unused
macros for these unsupported modes.

Signed-off-by: Pali Rohár <pali@kernel.org>
Fixes: 9695375a3f4a ("phy: add A3700 COMPHY support")
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/phy/marvell/phy-mvebu-a3700-comphy.c | 6 ------
 1 file changed, 6 deletions(-)

--- a/drivers/phy/marvell/phy-mvebu-a3700-comphy.c
+++ b/drivers/phy/marvell/phy-mvebu-a3700-comphy.c
@@ -33,18 +33,12 @@
 #define COMPHY_FW_MODE_USB3H			0x4
 #define COMPHY_FW_MODE_USB3D			0x5
 #define COMPHY_FW_MODE_PCIE			0x6
-#define COMPHY_FW_MODE_RXAUI			0x7
-#define COMPHY_FW_MODE_XFI			0x8
-#define COMPHY_FW_MODE_SFI			0x9
 #define COMPHY_FW_MODE_USB3			0xa
 
 #define COMPHY_FW_SPEED_1_25G			0 /* SGMII 1G */
 #define COMPHY_FW_SPEED_2_5G			1
 #define COMPHY_FW_SPEED_3_125G			2 /* 2500BASE-X */
 #define COMPHY_FW_SPEED_5G			3
-#define COMPHY_FW_SPEED_5_15625G		4 /* XFI 5G */
-#define COMPHY_FW_SPEED_6G			5
-#define COMPHY_FW_SPEED_10_3125G		6 /* XFI 10G */
 #define COMPHY_FW_SPEED_MAX			0x3F
 
 #define COMPHY_FW_MODE(mode)			((mode) << 12)
